{
  "type" : "CIMLayerDocument",
  "version" : "3.1.0",
  "build" : 41833,
  "layers" : [
    "CIMPATH=western_united_states/topography_slopesteepnessrating_tif.json"
  ],
  "layerDefinitions" : [
    {
      "type" : "CIMRasterLayer",
      "name" : "Slope Steepness Rating",
      "uRI" : "CIMPATH=western_united_states/topography_slopesteepnessrating_tif.json",
      "sourceModifiedTime" : {
        "type" : "TimeInstant"
      },
      "useSourceMetadata" : true,
      "description" : "Topography_SlopeSteepnessRating.tif",
      "layerElevation" : {
        "type" : "CIMLayerElevationSurface",
        "elevationSurfaceLayerURI" : "CIMPATH=Map/03c52e4f86344adba3ad725478394348.json"
      },
      "expanded" : true,
      "layerType" : "Operational",
      "showLegends" : true,
      "visibility" : true,
      "displayCacheType" : "Permanent",
      "maxDisplayCacheAge" : 5,
      "showPopups" : true,
      "serviceLayerID" : 1,
      "refreshRate" : -1,
      "refreshRateUnit" : "esriTimeUnitsSeconds",
      "blendingMode" : "Alpha",
      "allowDrapingOnIntegratedMesh" : true,
      "dataConnection" : {
        "type" : "CIMStandardDataConnection",
        "workspaceConnectionString" : "DATABASE=.\\TEMP_NewTopography",
        "workspaceFactory" : "Raster",
        "dataset" : "Topography_SlopeSteepnessRating.tif",
        "datasetType" : "esriDTAny"
      },
      "colorizer" : {
        "type" : "CIMRasterUniqueValueColorizer",
        "resamplingType" : "NearestNeighbor",
        "noDataColor" : {
          "type" : "CIMRGBColor",
          "values" : [
            255,
            255,
            255,
            0
          ]
        },
        "defaultColor" : {
          "type" : "CIMRGBColor",
          "values" : [
            0,
            255,
            0,
            100
          ]
        },
        "fieldName" : "SlopeDesc",
        "groups" : [
          {
            "type" : "CIMRasterUniqueValueGroup",
            "classes" : [
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "01 Level"
                ],
                "label" : "01 Level",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    25.199999999999999,
                    228.90000000000001,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "02 Nearly level"
                ],
                "label" : "02 Nearly level",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    50.399999999999999,
                    203.59999999999999,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "03 Very gentle slope"
                ],
                "label" : "03 Very gentle slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    76.299999999999997,
                    178.40000000000001,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "04 Gentle slope"
                ],
                "label" : "04 Gentle slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    101.8,
                    152.59999999999999,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "05 Moderate slope"
                ],
                "label" : "05 Moderate slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    127,
                    127,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "06 Strong slope"
                ],
                "label" : "06 Strong slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    152.59999999999999,
                    101.8,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "07 Very strong slope"
                ],
                "label" : "07 Very strong slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    178.40000000000001,
                    76.299999999999997,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "08 Extreme slope"
                ],
                "label" : "08 Extreme slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    203.59999999999999,
                    50.399999999999999,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "09 Steep slope"
                ],
                "label" : "09 Steep slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    228.90000000000001,
                    25.199999999999999,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              },
              {
                "type" : "CIMRasterUniqueValueClass",
                "values" : [
                  "10 Very steep slope"
                ],
                "label" : "10 Very steep slope",
                "color" : {
                  "type" : "CIMRGBColor",
                  "values" : [
                    255,
                    0,
                    0,
                    100
                  ]
                },
                "editable" : true,
                "visible" : true
              }
            ],
            "heading" : "SlopeDesc"
          }
        ],
        "colorRamp" : {
          "type" : "CIMMultipartColorRamp",
          "colorRamps" : [
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  0,
                  255,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  28,
                  226,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  28,
                  226,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  56,
                  198,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  56,
                  198,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  85,
                  170,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  85,
                  170,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  113,
                  141,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  113,
                  141,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  141,
                  113,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  141,
                  113,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  170,
                  85,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  170,
                  85,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  198,
                  56,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  198,
                  56,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  226,
                  28,
                  0,
                  100
                ]
              }
            },
            {
              "type" : "CIMLinearContinuousColorRamp",
              "fromColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  226,
                  28,
                  0,
                  100
                ]
              },
              "toColor" : {
                "type" : "CIMRGBColor",
                "values" : [
                  255,
                  0,
                  0,
                  100
                ]
              }
            }
          ],
          "weights" : [
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111,
            0.1111111111111111
          ]
        },
        "defaultLabel" : "<all other values>"
      },
      "attributeTable" : {
        "type" : "CIMRasterTable",
        "displayField" : "SlopePCT",
        "editable" : true
      }
    }
  ],
  "rGBColorProfile" : "sRGB IEC61966-2-1 noBPC",
  "cMYKColorProfile" : "U.S. Web Coated (SWOP) v2",
  "elevationSurfaceLayerDefinitions" : [
    {
      "type" : "CIMElevationSurfaceLayer",
      "name" : "Ground",
      "uRI" : "CIMPATH=Map/03c52e4f86344adba3ad725478394348.json",
      "useSourceMetadata" : true,
      "description" : "Ground",
      "expanded" : true,
      "layerType" : "Operational",
      "showLegends" : false,
      "visibility" : true,
      "displayCacheType" : "Permanent",
      "maxDisplayCacheAge" : 5,
      "showPopups" : true,
      "serviceLayerID" : -1,
      "refreshRate" : -1,
      "refreshRateUnit" : "esriTimeUnitsSeconds",
      "blendingMode" : "Alpha",
      "allowDrapingOnIntegratedMesh" : true,
      "elevationMode" : "BaseGlobeSurface",
      "verticalExaggeration" : 1,
      "color" : {
        "type" : "CIMRGBColor",
        "values" : [
          255,
          255,
          255,
          100
        ]
      },
      "surfaceTINShadingMode" : "Smooth"
    }
  ]
}